{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":20,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,"Emissions at manufacture","kgCO2","Emissions in operation"]
[null,null,null,"Year",0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[null,null,null,"New Diesel",8325,{"$f":"E4+$O$9","v":10173},{"$f":"F4+$O$9","v":12021},13869,15717,17565,19413,21261,23109,24957,26805,28653,30501,32349,34197,36045]
[null,null,null,"New Electric",13500,{"$f":"E5+$O$10","v":14068.4},14636.8,15205.199999999999,15773.599999999999,16341.999999999998,16910.399999999998,17478.8,18047.2,18615.600000000002,19184.000000000004,19752.400000000005,20320.800000000007,20889.200000000008,21457.600000000009,22026.000000000011]
[null,null,null,"Used Diesel",0,{"$f":"$O$9+E6","v":1848.0000000000002},{"$f":"$O$9+F6","v":3696.0000000000005},5544.0000000000009,7392.0000000000009,9240.0000000000018,11088.000000000002,12936.000000000002,14784.000000000002,16632.000000000004,18480.000000000004,20328.000000000004,22176.000000000004,24024.000000000004,25872.000000000004,27720.000000000004]
[null,null,null,"Used Electric",0,{"$f":"$O$10+E7","v":568.40000000000009},{"$f":"$O$10+F7","v":1136.8000000000002},1705.2000000000003,2273.6000000000004,2842.0000000000005,3410.4000000000005,3978.8000000000006,4547.2000000000007,5115.6000000000004,5684,6252.4,6820.7999999999993,7389.1999999999989,7957.5999999999985,8525.9999999999982]
[{"$nulls":7},"Fuel econ.",null,"Emissions",null,"Distance"]
[null,null,null,"Fuel","2.64 kg CO2/litre diesel burned",null,null,5,"l/100",2.64,"kg/l",14000,"km/yr",null,{"$f":"H9*J9*L9/100","v":1848.0000000000002},"kg CO2 pa"]
[null,null,null,"Grid","0.58 kgCO2/kWh consumed",null,null,14.5,"kWh/100",0.28000000000000003,"kg/kWh",14000,"km/yr",null,{"$f":"H10*J10*L10/100","v":568.40000000000009},"kg CO2 pa"]
[]
[]
[{"$nulls":18},7]
[]
[]
[{"$nulls":17},1,5,{"$f":"R16*S16/$S$13","v":0.7142857142857143}]
[{"$nulls":17},2,4,{"$f":"R17*S17/$S$13","v":1.1428571428571428}]
[{"$nulls":17},3,6,2.5714285714285716]
[{"$nulls":17},4,3,1.7142857142857142]
[{"$nulls":17},5,7,{"$f":"R20*S20/$S$13","v":5}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}